***Supreme Tilt & Turn window***



Superior insulation, dual weather seals and a multi-chambered design reduce heat loss and noise infiltration so that your family can enjoy warmer, more comfortable living. The fusion welded frame and corners ensure strength, stability and long-lasting durability, while the multi-point locking system around the entire frame offers total security whether closed or tilted open.

|  |
| --- |
| **FRAME – Fusion welded corners** |
| White extruded polyvinyl chloride (uPVC) profiles. Optional permafinish colors available |
| Operator/Fixed Frame depth: 3.25” (83mm)  |
| **SASH** |
| The sash measures 2.375” from inside to outside |
| **GLAZING** |
| **Glazing method** | Insulated glass, hermetically sealed |
| **Glazing seal** | Compression seal, silicon heel bead |
| **Spacer type** | Warm edge intercept, Ultra or SuperSpacer |
| **Options** | High Solar Gain LoE, Low Solar Gain LoE, Argon gas fill, Obscure glass, Tinted glass,Energlas (LoE/Argon and Ultra spacer),Energlas Plus (triple paned, 2 panes with LoE glass, argon gas filling and Superspacer) |
| **OPTIONS** |
| **Insect Screens** | Aluminum framed full screen standard, white or matched to frame and sashGrey fiberglass standard screen mesh with pull tabs integrated into screen corner |
| **SDL – Simulated Divided Lites** | Int. bar: Extruded vinyl or wood, 7/8” and 1 1/8” wide bars. Ext. bar: Extruded vinyl, 7/8” or 1 1/8” wide bars. White, tan or paintedPattern: Rectangular, Craftsman, Prairie , custom lite layouts available  |
| **Grills** | ¾” Contoured Georgian. White, tan, brushed aluminum, painted, split finish int/ext1” Contoured Georgian. White, painted, split finish int/ext5/8” Flat Colonial. White, tan, brass, brushed aluminum, painted, split finish int/extSlimline 5/16” Flat Colonial. White, tan, pewter, black, gold, mill finish or painted |
| **Accessories** | Optional: Add on ½” to ¾” interior return Optional: 7/8”, 1 ½”, 2” or 3 ½” brick molding all four sides or with subsill. All available with J-trim and nailing fin. 2” and 3 ½” available with decorative molding |
| **HARDWARE** |
| Roto NT Euro-groove | Fully adjustable hinges |
| Multiple locking points | All hardware is stainless steel |
| Operating panels are fitted with a handle mounted on the sash at a location relative to the panel height | Operating handle powder coated white or ttanium |

|  |
| --- |
| **PERFORMANCE TESTS In accordance with AAMA/WDMA/CSA 101/1.5.2/A444-08** |
| **Window****(Supreme)** | **Gateway Size (in)** | **Gateway Size (mm)** | **NAFS** **Rating** | **Canadian Air Infiltration** | **Water Resistance** | **Wind Load Resistance** | **DP Rating**  |
| **Water** | **Wind** |
| **T & T**  | 44 x 60 | 1118 x 1524 | R-PG50 | A3 | B7 | C5 | N/A | N/A |
| **T & T Fixed Sash** | 48 x 48 | 1219 x 1219 | R-PG50 | FX | B7 | C5 | N/A | N/A |
| **T & T Picture** | 72 x 72 | 1829 x 1829 | CW-PG65-FW | N/A | N/A | N/A | DP100 | DP65 |

|  |  |
| --- | --- |
|  | **THERMAL PERFORMANCE RATINGS In accordance to CSA A440.2-04** |
| **Glass Options** | **Energy Rating** | **R-Value (Whole Window)** | **R-Value (Center of Glass)** | **U-Value (metric)** | **U-Value (imperial)** | **Solar Heat Gain Coefficient** | **Visible Transmittance** | **Condensation Resistance** | **Canadian Energy Star Zones** | **US Energy****Star Zones** |
| **Double Glazed** | Energlas – HSG | 31 | 3.45 | 3.69 | 1.6 | 0.29 | 0.48 | 0.54 | 62 | ABC | N |
| LoE/Argon – HSG | 31 | 3.45 | 3.69 | 1.6 | 0.29 | 0.48 | 0.54 | 61 | ABC | N |
| LoE/Argon – HSG w Grills | 28 | 3.45 | 3.69 | 1.6 | 0.29 | 0.42 | 0.48 | 61 | AB | N |
| Energlas – HSG w Grills | 28 | 3.45 | 3.69 | 1.6 | 0.29 | 0.42 | 0.48 | 62 | AB | N |
| Energlas – LSG | 22 | 3.70 | 4.10 | 1.5 | 0.27 | 0.27 | 0.48 | 64 | AB | N,NC,SC,S |
| LoE/Argon – LSG | 20 | 3.57 | 4.10 | 1.6 | 0.28 | 0.27 | 0.48 | 62 | AB | N,NC,SC,S |
| Energlas – LSG w Grills | 20 | 3.70 | 4.10 | 1.5 | 0.27 | 0.24 | 0.42 | 64 | AB | N,NC,SC,S |
| LoE/Argon – LSG w Grills | 19 | 3.57 | 4.10 | 1.6 | 0.28 | 0.24 | 0.42 | 62 | AB | N,NC,SC,S |
| Clear | 16 | 2.33 | 2.08 | 2.4 | 0.43 | 0.42 | 0.55 | 45 |   |  |
| Clear w Grills | 13 | 2.33 | 2.08 | 2.4 | 0.43 | 0.46 | 0.48 | 45 |   |  |
| **Triple Glazed** |   |   |   |  |   |   |   |   |   |   |  |
| Energlas Plus Argon – HSG | 38 | 5.00 | 6.85 | 1.1 | 0.2 | 0.41 | 0.49 | 68 | ABCD |  |
| Energlas Plus Argon – LSG | 28 | 5.26 | 7.94 | 1.1 | 0.19 | 0.21 | 0.38 | 68 | ABCD |  |
| Triple LoE/Argon x 1 LSG | 25 | 4.35 | 5.26 | 1.3 | 0.23 | 0.25 | 0.44 | 69 | ABC | N,NC,SC,S |
|   | \***Energlas** uses a high performance warm edge spacer, one panel of LoE coated glass and one cavity filled with high density gas. |  |
|   | \*\***Energlas Plus** is an ultra high performance, energy efficient, triple glazed system using warm edge SuperSpacer, two panels of LoE coated glass, and two cavities filled with high density glass. |  |