***Supreme Double Hung***



Watch your home take on an outstanding level of character and charm. Supreme Double Hung are made from tough, durable vinyl and available in a range of designer colors. Supreme Double Hung are practical too. Engineered to provide a high degree of ventilation with features like a stainless steel coil spring balance system and Intercept warm edge spacers. Both top and bottom sashes tilt in for easy cleaning.

|  |
| --- |
| **FRAME – Fusion welded corners** |
| White extruded polyvinyl chloride (uPVC) profiles. Optional tan extrusion, permafinish paint colors available |
| Operator/Fixed Frame depth: 3.25” (83mm)  |
| Picture Window Frame depth: 3.25” (83mm) |
| **SASH – Fusion welded corners** |
| White extruded polyvinyl chloride (uPVC) profiles. Optional tan extrusion, permafinish paint colors available |
| **GLAZING** |
| **Glazing method** | Insulated glass, hermetically sealed, dual seal |
| **Glazing seal** | Tape glazed, silicon heel bead |
| **Spacer type** | Warm edge intercept, Ultra or SuperSpacer |
| **Options** | High Solar Gain LoE, Low Solar Gain LoE, Argon gas fill, Obscure glass, Tinted glass,Energlas (LoE/Argon and Ultra spacer),Energlas Plus (triple paned, 2 panes with LoE glass, argon gas filling and Superspacer) |
| **WEATHER STRIPPING** |
| **Dual sealed** | Dual weather pile weather strip with sealing fin. Color: grey |
| **OPTIONS** |
| **Insect Screens** | Aluminum bar full or half screen, white or tan to match frame and sashGrey fiberglass standard screen mesh with pull tabs integrated into screen corner |
| **SDL – Simulated Divided Lites** | Int. bar: Extruded vinyl or wood, 7/8” and 1 1/8” wide bars. Ext. bar: Extruded vinyl, 7/8” or 1 1/8” wide bars. White, tan or paintedPattern: Rectangular, Craftsman, Prairie , custom lite layouts available  |
| **Grills** | ¾” Contoured Georgian. White, tan, brushed aluminum, painted, split finish int/ext1” Contoured Georgian. White, painted, split finish int/ext5/8” Flat Colonial. White, tan, brass, brushed aluminum, painted, split finish int/extSlimline 5/16” Flat Colonial. White, tan, pewter, black, gold, mill finish or painted |
| **Accessories** | Optional: Add-on ½” to ¾” return on the interior Optional: 7/8”, 1 ½”, 2” or 3 ½” brick molding all four sides or with subsill. All available with J-trim and nailing fin. 2” and 3 ½” available with decorative molding |
| **HARDWARE** |
| Truth camlock and keeper | John Evans constant force balance |
| Stainless pivot bars | Auto engage night lock |

|  |
| --- |
| **PERFORMANCE TESTS In accordance with AAMA/WDMA/CSA 101/1.5.2/A444-08** |
| **Window (Supreme)** | **Gateway Size (in)** | **Gateway Size (mm)** | **NAFS Rating** | **Canadian Air Infiltration** | **Water Resistance** | **Wind Load Resistance** | **DP Rating** |
| **Water** | **Wind** |
| **Double Hung** | 39 x 63 | 991 x 1600 | N/A | N/A | B3 | C4 | DP50 | DP65 |
| 40 x 63 | 1016 x 1600 | R-PG50-H | A3 | B3 | C4 | DP50 | DP65 |
| **Double Hung Picture** | 78 7/8 x 78 7/8 | 2003 x 2003 | N/A | FX | B7 | C5 | N/A | N/A |
| 50 x 100 | 1270 x 2540 | R-PG50-FW | FX | B7 | C3 | N/A | N/A |
| 72 x 84 | 1829 x 2134 | CW-PG60-FW | FX | B7 | C4 | N/A | N/A |
| **Double Glider** | 63 x 44 | 1600 x 1118 | R-PG45-HS | A2 | B3 | C4 | DP45 | DP55 |

|  |  |
| --- | --- |
|  | **THERMAL PERFORMANCE RATINGS In accordance to CSA A440.2-04** |
| **Glass Options** | **Energy Rating** | **R-Value (Whole Window)** | **R-Value (Center of Glass)** | **U-Value (metric)** | **U-Value (imperial)** | **Solar Heat Gain Coefficient** | **Visible Transmittance** | **Condensation Resistance** | **Canadian Energy Star Zones** | **US Energy****Star Zones** |
| **Double Glazed** | Energlas – HSG | 30 | 3.13 | 3.69 | 1.8 | 0.32 | 0.53 | 0.6 | 57 | ABC | N |
| LoE/Argon – HSG | 30 | 3.13 | 3.69 | 1.8 | 0.32 | 0.53 | 0.6 | 55 | ABC | N |
| LoE/Argon – HSG w Grills | 27 | 3.13 | 3.69 | 1.8 | 0.32 | 0.47 | 0.54 | 55 | AB | N |
| Energlas – HSG w Grills | 27 | 3.13 | 3.69 | 1.8 | 0.32 | 0.47 | 0.54 | 57 | AB | N |
| Energlas – LSG | 19 | 3.33 | 4.10 | 1.7 | 0.30 | 0.29 | 0.53 | 58 | A | N,NC,SC |
| LoE/Argon – LSG | 17 | 3.23 | 4.10 | 1.8 | 0.31 | 0.29 | 0.53 | 56 | A | NC,SC |
| Energlas – LSG w Grills | 17 | 3.33 | 4.10 | 1.7 | 0.30 | 0.29 | 0.47 | 58 | A | N,NC,SC,S |
| LoE/Argon – LSG w Grills | 16 | 3.23 | 4.10 | 1.8 | 0.31 | 0.26 | 0.47 | 56 | A | NC,SC,S |
| Clear | 14 | 2.13 | 2.08 | 2.7 | 0.47 | 0.57 | 0.61 | 47 |   |  |
| Clear w Grills | 10 | 2.13 | 2.08 | 2.7 | 0.47 | 0.51 | 0.54 | 47 |   |  |
| **Triple Glazed** |   |   |   |  |   |   |   |   |   |   |  |
| Energlas Plus Krypton – HSG | 37 | 4.35 | 6.85 | 1.3 | 0.23 | 0.45 | 0.54 | 62 | ABCD |  |
| Energlas Plus Argon – HSG | 32 | 3.70 | 4.74 | 1.5 | 0.27 | 0.45 | 0.54 | 62 | ABC | N |
| Energlas Plus Krypton – LSG | 26 | 4.76 | 7.94 | 1.2 | 0.21 | 0.23 | 0.41 | 63 | ABCD |  |
| Energlas Plus Argon – LSG | 21 | 3.85 | 5.13 | 1.5 | 0.26 | 0.24 | 0.41 | 62 | AB | N,NC,SC,S |
| Triple Clear | 20 | 2.56 | 3.21 | 2.2 | 0.39 | 0.51 | 0.55 | 52 |   |  |
| Triple LoE/Argon x 1 LSG | 17 | 3.23 | 5.26 | 1.8 | 0.31 | 0.28 | 0.48 | 60  |  A | NC,SC |
|   | \***Energlas** uses a high performance warm edge spacer, one panel of LoE coated glass and one cavity filled with high density gas. |  |
|   | \*\***Energlas Plus** is an ultra high performance, energy efficient, triple glazed system using warm edge SuperSpacer, two panels of LoE coated glass, and two cavities filled with high density glass. |  |